###############################################################################
# $Id: pptpd-options 4643 2006-11-06 18:42:43Z rene $
#
# Sample Poptop PPP options file /etc/ppp/pptpd-options
# Options used by PPP when a connection arrives from a client.
# This file is pointed to by /etc/pptpd.conf option keyword.
# Changes are effective on the next connection.  See "man pppd".
#
# You are expected to change this file to suit your system.  As
# packaged, it requires PPP 2.4.2 and the kernel MPPE module.
###############################################################################


# Authentication
auth
# Name of the local system for authentication purposes 
# (must match the second field in /etc/ppp/chap-secrets entries)
name pptpd

# Optional: domain name to use for authentication
# domain mydomain.net

# Strip the domain prefix from the username before authentication.
# (applies if you use pppd with chapms-strip-domain patch)
#chapms-strip-domain


# Encryption
# Debian: on systems with a kernel built with the package
# kernel-patch-mppe >= 2.4.2 and using ppp >= 2.4.2, ...
# {{{
refuse-pap
refuse-chap
refuse-mschap
# Require the peer to authenticate itself using MS-CHAPv2 [Microsoft
# Challenge Handshake Authentication Protocol, Version 2] authentication.
require-mschap-v2
# Require MPPE 128-bit encryption
# (note that MPPE requires the use of MSCHAP-V2 during authentication)
require-mppe-128
# }}}




# Network and Routing

# If pppd is acting as a server for Microsoft Windows clients, this
# option allows pppd to supply one or two DNS (Domain Name Server)
# addresses to the clients.  The first instance of this option
# specifies the primary DNS address; the second instance (if given)
# specifies the secondary DNS address.
# Attention! This information may not be taken into account by a Windows
# client. See KB311218 in Microsoft's knowledge base for more information.
#ms-dns 10.0.0.1
#ms-dns 10.0.0.2

# If pppd is acting as a server for Microsoft Windows or "Samba"
# clients, this option allows pppd to supply one or two WINS (Windows
# Internet Name Services) server addresses to the clients.  The first
# instance of this option specifies the primary WINS address; the
# second instance (if given) specifies the secondary WINS address.
#ms-wins 10.0.0.3
#ms-wins 10.0.0.4

# Add an entry to this system's ARP [Address Resolution Protocol]
# table with the IP address of the peer and the Ethernet address of this
# system.  This will have the effect of making the peer appear to other
# systems to be on the local ethernet.
# (you do not need this if your PPTP server is responsible for routing
# packets to the clients -- James Cameron)
proxyarp

# Debian: do not replace the default route
nodefaultroute


# Logging

# Enable connection debugging facilities.
# (see your syslog configuration for where pppd sends to)
#debug

# Print out all the option values which have been set.
# (often requested by mailing list to verify options)
#dump


# Miscellaneous

# Create a UUCP-style lock file for the pseudo-tty to ensure exclusive
# access.
lock

# Disable BSD-Compress compression
nobsdcomp 
